<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<schematic>
<libraries>
<library name="microchip-pic18fxx5x">
<packages>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type SP</description>
</package>
</packages>
<symbols>
<symbol name="PIC18F2550">
<pin name="_MCLR/VPP/RE3" direction="in"/>
<pin name="AN0/RA0"/>
<pin name="AN1/RA1"/>
<pin name="VREF-/CVREF/AN2/RA2"/>
<pin name="VREF+/AN3/RA3"/>
<pin name="RCV/T0CKI/C1OUT/RA4"/>
<pin name="_SS/HLVDIN/C2OUT/AN4/RA5"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="OSC1/CLKI/RA7"/>
<pin name="OSC2/CLKO/RA6"/>
<pin name="T1OSO/T13CKI/RC0"/>
<pin name="_UOE/T1OSI/CCP2/RC1"/>
<pin name="CCP1/RC2"/>
<pin name="VUSB"/>
<pin name="D-/VM/RC4"/>
<pin name="D+/VP/RC5"/>
<pin name="TX/CK/RC6"/>
<pin name="SDO/RX/DT/RC7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT0/FLT0/SDI/SDA/AN12/RB0"/>
<pin name="INT1/SCK/SCL/AN10/RB1"/>
<pin name="INT2/VMO/AN8/RB2"/>
<pin name="CCP2/VPO/AN9/RB3"/>
<pin name="KBI0/AN11/RB4"/>
<pin name="KBI1/PGM/RB5"/>
<pin name="KBI2/PGC/RB6"/>
<pin name="KBI3/PGD/RB7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PIC18*2550">
<description>&lt;B&gt;PIC18*2550 Microchip FLASH Microcontroller with FS-USB&lt;/B&gt;
&lt;p&gt;
&lt;HR&gt;
&lt;B&gt;DEVICE FEATURES&lt;/B&gt;&lt;br&gt;
&lt;table border=1 bgcolor=#ffffff align=center&gt;
&lt;tr bgcolor=#CCCCCC&gt;
&lt;td &gt;Feature&lt;/td&gt;&lt;td align=center&gt;PIC18*2550 &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Program Memory (bytes) &lt;/td&gt;&lt;td align=center&gt;32k &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Program Memory (instructions) &lt;/td&gt;&lt;td align=center&gt;16384 &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;I/O Ports &lt;/td&gt;&lt;td align=center&gt;Ports A, B, C, (E) &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Capture/Compare/PWM Modules &lt;/td&gt;&lt;td align=center&gt;2&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Enhanced Capture/Compare/PWM Modules &lt;/td&gt;&lt;td align=center&gt;0&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Parallel Communications (PSP) &lt;/td&gt;&lt;td align=center&gt;No &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;10-bit Analog-to-Digital Module &lt;/td&gt;&lt;td align=center&gt;10 input Channels &lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td  bgcolor=#EEEEEE&gt;Package Types &lt;/td&gt;
&lt;td align=center&gt;28-pin PDIP&lt;br&gt;28-pin SOIC &lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;br&gt;
&lt;br&gt;&lt;B&gt;NOTES:&lt;/B&gt;
&lt;br&gt; F only after 18, means standard voltage range from 4.2v to 5.5v
&lt;br&gt; LF after 18, means extended voltage range from 2.0v to 5.5v
&lt;br&gt; T after entire device number, means supplied in tape and reel TQFP packages only
&lt;br&gt; -E before / denotes extended temperature range from -40&amp;deg;C  to +120&amp;deg;C
&lt;br&gt; -I before / denotes industrial temperature range from -40&amp;deg;C  to +85&amp;deg;C
&lt;br&gt; /PT suffix denotes TQFP package
&lt;br&gt; /SO suffix denotes SOIC package
&lt;br&gt; /SP suffix denotes Skinny Plastic DIP package
&lt;br&gt; /P suffix denotes Plastic DIP package
&lt;br&gt; /ML suffix denotes QFN package</description>
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="-I/SO" package="SO-28W">
<connects>
<connect gate="G$1" pin="AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="CCP2/VPO/AN9/RB3" pad="24"/>
<connect gate="G$1" pin="D+/VP/RC5" pad="16"/>
<connect gate="G$1" pin="D-/VM/RC4" pad="15"/>
<connect gate="G$1" pin="INT0/FLT0/SDI/SDA/AN12/RB0" pad="21"/>
<connect gate="G$1" pin="INT1/SCK/SCL/AN10/RB1" pad="22"/>
<connect gate="G$1" pin="INT2/VMO/AN8/RB2" pad="23"/>
<connect gate="G$1" pin="KBI0/AN11/RB4" pad="25"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="26"/>
<connect gate="G$1" pin="KBI2/PGC/RB6" pad="27"/>
<connect gate="G$1" pin="KBI3/PGD/RB7" pad="28"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="10"/>
<connect gate="G$1" pin="RCV/T0CKI/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SDO/RX/DT/RC7" pad="18"/>
<connect gate="G$1" pin="T1OSO/T13CKI/RC0" pad="11"/>
<connect gate="G$1" pin="TX/CK/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VREF-/CVREF/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="VSS@0" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
<connect gate="G$1" pin="_MCLR/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="_SS/HLVDIN/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="_UOE/T1OSI/CCP2/RC1" pad="12"/>
</connects>
<technologies>
<technology name="F"/>
<technology name="LF"/>
</technologies>
</device>
<device name="-I/SP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AN0/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/RA1" pad="3"/>
<connect gate="G$1" pin="CCP1/RC2" pad="13"/>
<connect gate="G$1" pin="CCP2/VPO/AN9/RB3" pad="24"/>
<connect gate="G$1" pin="D+/VP/RC5" pad="16"/>
<connect gate="G$1" pin="D-/VM/RC4" pad="15"/>
<connect gate="G$1" pin="INT0/FLT0/SDI/SDA/AN12/RB0" pad="21"/>
<connect gate="G$1" pin="INT1/SCK/SCL/AN10/RB1" pad="22"/>
<connect gate="G$1" pin="INT2/VMO/AN8/RB2" pad="23"/>
<connect gate="G$1" pin="KBI0/AN11/RB4" pad="25"/>
<connect gate="G$1" pin="KBI1/PGM/RB5" pad="26"/>
<connect gate="G$1" pin="KBI2/PGC/RB6" pad="27"/>
<connect gate="G$1" pin="KBI3/PGD/RB7" pad="28"/>
<connect gate="G$1" pin="OSC1/CLKI/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKO/RA6" pad="10"/>
<connect gate="G$1" pin="RCV/T0CKI/C1OUT/RA4" pad="6"/>
<connect gate="G$1" pin="SDO/RX/DT/RC7" pad="18"/>
<connect gate="G$1" pin="T1OSO/T13CKI/RC0" pad="11"/>
<connect gate="G$1" pin="TX/CK/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VREF+/AN3/RA3" pad="5"/>
<connect gate="G$1" pin="VREF-/CVREF/AN2/RA2" pad="4"/>
<connect gate="G$1" pin="VSS@0" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
<connect gate="G$1" pin="_MCLR/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="_SS/HLVDIN/C2OUT/AN4/RA5" pad="7"/>
<connect gate="G$1" pin="_UOE/T1OSI/CCP2/RC1" pad="12"/>
</connects>
<technologies>
<technology name="F"/>
<technology name="LF"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT54E">
<description>&lt;b&gt;SOT-54&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
<symbols>
<symbol name="IGFNA">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BS170" prefix="Q">
<description>&lt;b&gt;N-CHANNEL MOS FET&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="IGFNA"/>
</gates>
<devices>
<device name="" package="SOT54E">
<connects>
<connect gate="1" pin="D" pad="D"/>
<connect gate="1" pin="G" pad="G"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rcl">
<packages>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5664</description>
</package>
<package name="HPC0201">
<description>&lt;b&gt; &lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/10129/hpc0201a.pdf</description>
</package>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
<package name="CT3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Reflow solder</description>
</package>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Reflow solder&lt;/b&gt;</description>
</package>
<package name="E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Reflow solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_Z">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_P">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SANYO-OSCON_9E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_9F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_A">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_D">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E1">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E9">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F0">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_G">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_H">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_A5">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_B6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC 1005 chip</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC 1310 chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC 1608 chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC 2012 chip&lt;br&gt;
Pad definition corrected 2006.05.15, librarian@cadsoft.de</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
IPC 3216 chip</description>
</package>
<package name="SANYO-OSCON_A'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="L2012C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC chip</description>
</package>
<package name="L2825P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC precision wire wound</description>
</package>
<package name="L3216C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC chip</description>
</package>
<package name="L3225M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC molded</description>
</package>
<package name="L3225P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC precision wire wound</description>
</package>
<package name="L3230M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC molded</description>
</package>
<package name="L4035M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
IPC molded</description>
</package>
<package name="L4516C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="L4532M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L4532P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="L5038P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt; &lt;p&gt;
precision wire wound</description>
</package>
<package name="L5650M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt; &lt;p&gt;
molded</description>
</package>
<package name="L8530M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt; &lt;p&gt;
molded</description>
</package>
<package name="L1812">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TJ3-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ3-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ4-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ4-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ5-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ5-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ6-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ6-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ7-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ7-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ8-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ8-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ9-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ9-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="POWER-CHOKE_WE-TPC">
<description>&lt;b&gt;POWER-CHOKE WE-TPC&lt;/b&gt;&lt;p&gt;
Würth Elektronik, Partnumber: 744053220&lt;br&gt;
Source: WE-TPC 744053220.pdf</description>
</package>
<package name="CEP125">
<description>&lt;b&gt;POWER INDUCTORS&lt;/b&gt; (SMT Type)&lt;p&gt;
Source: www.sumida.com/products/pdf/CEP125.pdf</description>
</package>
<package name="L0201">
<description>&lt;b&gt;NIS02 Chip Inductor&lt;/b&gt;&lt;p&gt;
Source: http://www.niccomp.com/Catalog/nis.pdf</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
IPC 1005 chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
IPC 1608 chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
IPC 2012 chip&lt;br&gt;
Pad definition corrected 2006.05.15, librarian@cadsoft.de</description>
</package>
<package name="R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Pad definition corrected 2006.05.15, librarian@cadsoft.de</description>
</package>
<package name="R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
IPC 3216 chip</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
IPC 3225 chip</description>
</package>
</packages>
<symbols>
<symbol name="R-EU">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CPOL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="L-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HPC0201" package="HPC0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0201" package="C0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CPOL-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="CPOL"/>
</gates>
<devices>
<device name="CT3216" package="CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT3528" package="CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6032" package="CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT7343" package="CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181A" package="B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181B" package="B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181C" package="B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181D" package="B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4" package="TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4L" package="TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5" package="TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6" package="TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6L" package="TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7L" package="TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7" package="TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D10" package="TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11" package="TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11L" package="TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT6D6" package="TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D6L" package="TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7" package="TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7L" package="TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9" package="TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9L" package="TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR1" package="ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR2" package="ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR3" package="ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR4" package="ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR5" package="ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-35" package="P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-40" package="P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-50" package="P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-60" package="P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-45" package="TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-50" package="TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-70" package="TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-60" package="TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-80" package="TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E1.8-4" package="E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-5AXIAL" package="E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-6AXIAL" package="E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-9AXIAL" package="E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5V" package="E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5" package="E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-6" package="E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-7" package="E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-4V" package="E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-4" package="E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-5" package="E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-10AXIAL" package="E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-6AXIAL" package="E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-9AXIAL" package="E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-10" package="E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-10AXIAL" package="E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-9AXIAL" package="E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-8" package="E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-10AXIAL" package="E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-12AXIAL" package="E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-16AXIAL" package="E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-12AXIAL" package="E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-14AXIAL" package="E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-16AXIAL" package="E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-18AXIAL" package="E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-16AXIAL" package="E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-18AXIAL" package="E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-21AXIAL" package="E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-22AXIAL" package="E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-25AXIAL" package="E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-10.5" package="E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-13" package="E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-4" package="E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-5" package="E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-6" package="E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-8.5" package="E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-25AXIAL" package="E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-30AXIAL" package="E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-25AXIAL" package="E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-30AXIAL" package="E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-9VAXIAL" package="E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-16" package="E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-18" package="E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-20" package="EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-22.5" package="EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-25" package="EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-30" package="EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-35" package="EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1R" package="085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1W" package="085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AR" package="085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AW" package="085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2R" package="139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2W" package="139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3R" package="139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3W" package="139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-0810" package="140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1010" package="140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1014" package="140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-0810" package="150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1010" package="150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1014" package="150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0405" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0505" package="153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0605" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0807" package="153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0810" package="153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1010" package="153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1012" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1014" package="153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0808" package="175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0810" package="175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18R" package="A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18W" package="A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21R" package="B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21W" package="B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28R" package="C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28W" package="C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31R" package="D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31W" package="D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38R" package="E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38W" package="E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12R" package="R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12W" package="R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5L" package="TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2,5-6E" package="E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCA" package="SMC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCZ" package="SMC_Z">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCP" package="SMC_P">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCB" package="SMC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCC" package="SMC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCD" package="SMC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMCE" package="SMC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_9E" package="SANYO-OSCON_9E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_9F" package="SANYO-OSCON_9F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_A" package="SANYO-OSCON_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_A'" package="SANYO-OSCON_A'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_B" package="SANYO-OSCON_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_B'" package="SANYO-OSCON_B'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C" package="SANYO-OSCON_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C'" package="SANYO-OSCON_C'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_C6" package="SANYO-OSCON_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_D" package="SANYO-OSCON_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E" package="SANYO-OSCON_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E'" package="SANYO-OSCON_E'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E1" package="SANYO-OSCON_E1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E12" package="SANYO-OSCON_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E13" package="SANYO-OSCON_E13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E7" package="SANYO-OSCON_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_E9" package="SANYO-OSCON_E9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F" package="SANYO-OSCON_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F'" package="SANYO-OSCON_F'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F0" package="SANYO-OSCON_F0">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F13" package="SANYO-OSCON_F13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_F8" package="SANYO-OSCON_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_G" package="SANYO-OSCON_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_H" package="SANYO-OSCON_H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_A5" package="SANYO-OSCON_SMD_A5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_B6" package="SANYO-OSCON_SMD_B6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_C6" package="SANYO-OSCON_SMD_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_E12" package="SANYO-OSCON_SMD_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_E7" package="SANYO-OSCON_SMD_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_F12" package="SANYO-OSCON_SMD_F12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SANYO_SMD_F8" package="SANYO-OSCON_SMD_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-US" prefix="L" uservalue="yes">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="L2012C" package="L2012C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L2825P" package="L2825P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3216C" package="L3216C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3225M" package="L3225M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3225P" package="L3225P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3230M" package="L3230M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4035M" package="L4035M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4516C" package="L4516C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4532C" package="L4532M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4532P" package="L4532P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L5038P" package="L5038P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L5650M" package="L5650M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L8530M" package="L8530M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L1812" package="L1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ3-U1" package="TJ3-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ3-U2" package="TJ3-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ4-U1" package="TJ4-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ4-U2" package="TJ4-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ5-U1" package="TJ5-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ5-U2" package="TJ5-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ6-U1" package="TJ6-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ6-U2" package="TJ6-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ7-U1" package="TJ7-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ7-U2" package="TJ7-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ8-U1" package="TJ8-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ8-U2" package="TJ8-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ9-U1" package="TJ9-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ9-U2" package="TJ9-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WE-TPC" package="POWER-CHOKE_WE-TPC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CEP125" package="CEP125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L0201" package="L0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="R-EU"/>
</gates>
<devices>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/2V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0201" package="R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply">
<packages>
</packages>
<symbols>
<symbol name="VDD">
<pin name="VDD" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VDD" prefix="V">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VDD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49GW">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49TL-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-LM">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U70">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC13U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="86SMX">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="MM20SS">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="MM39SL">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CRYSTAL" prefix="Q" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="HC49S" package="HC49/S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49GW" package="HC49GW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49TL-H" package="HC49TL-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U-H" package="HC49U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U-LM" package="HC49U-LM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U-V" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U70" package="HC49U70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC13U-H" package="HC13U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC18U-H" package="HC18U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC18U-V" package="HC18U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC33U-H" package="HC33U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC33U-V" package="HC33U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM49" package="SM49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC26H" package="TC26H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC26V" package="TC26V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC38H" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="68SMX" package="86SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MM20SS" package="MM20SS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MM39SL" package="MM39SL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CTS406" package="CTS406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="diode">
<packages>
<package name="DO13M">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 6.35 mm metall, horizontal, grid 20.32 mm</description>
</package>
<package name="C4111-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.3 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="P6T15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 9 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="CB429-17">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5 mm, horizontal, grid 17 mm</description>
</package>
<package name="DO201T15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.6 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="F126Z12">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3 mm, horizontal, grid 12.7 mm</description>
</package>
<package name="AG">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 9 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="TO92H">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead plastic, vertical</description>
</package>
<package name="CB417-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3.5 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="CB429-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SMC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SCHOTTKY-DIODE" prefix="D" uservalue="yes">
<description>Schottky Diode</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="DO13M" package="DO13M">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4111-15" package="C4111-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P6T15" package="P6T15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB429-17" package="CB429-17">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO201T15" package="DO201T15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO35-7" package="DO35-7">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F126Z12" package="F126Z12">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AG" package="AG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92H" package="TO92H">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB417-15" package="CB417-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB429-15" package="CB429-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMC" package="SMC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-usb">
<packages>
<package name="USB-MB-S">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-H">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-HU">
<description>&lt;b&gt;USB Series A Hole Mounted Up-Right&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
</packages>
<symbols>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USB" prefix="X">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-MB-S" package="USB-MB-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-H" package="USB-B-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-HU" package="USB-A-HU">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp-quick">
<packages>
<package name="06PA">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MA06" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="" package="06PA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="V4" library="supply" deviceset="VDD" device=""/>
<part name="V5" library="supply" deviceset="VDD" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="X2" library="con-usb" deviceset="USB" device="-B-H"/>
<part name="V1" library="supply" deviceset="VDD" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="L2" library="rcl" deviceset="L-US" device="0207/10" value="100k"/>
<part name="U$2" library="microchip-pic18fxx5x" deviceset="PIC18*2550" device="-I/SP" technology="LF"/>
<part name="C6" library="rcl" deviceset="C-EU" device="050-024X044" value="100n"/>
<part name="C9" library="rcl" deviceset="C-EU" device="050-024X044" value="470n"/>
<part name="C7" library="rcl" deviceset="C-EU" device="050-024X044" value="22p"/>
<part name="C8" library="rcl" deviceset="C-EU" device="050-024X044" value="22p"/>
<part name="D1" library="diode" deviceset="SCHOTTKY-DIODE" device="DO35-7"/>
<part name="D2" library="diode" deviceset="SCHOTTKY-DIODE" device="DO35-7"/>
<part name="R2" library="rcl" deviceset="R-EU_" device="0207/10" value="5k5"/>
<part name="T1" library="transistor-small-signal" deviceset="BS170" device=""/>
<part name="T2" library="transistor-small-signal" deviceset="BS170" device=""/>
<part name="C1" library="rcl" deviceset="CPOL-EU" device="E3.5-10" value="200u"/>
<part name="R1" library="rcl" deviceset="R-EU_" device="0207/10" value="2k7"/>
<part name="R3" library="rcl" deviceset="R-EU_" device="0207/10" value="4k7"/>
<part name="Q1" library="crystal" deviceset="CRYSTAL" device="HC49S" value="20MHz"/>
<part name="C3" library="rcl" deviceset="CPOL-EU" device="E2,5-6E" value="22u"/>
<part name="C2" library="rcl" deviceset="CPOL-EU" device="E2,5-6E" value="22u"/>
<part name="ICSP" library="con-amp-quick" deviceset="MA06" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>FB</text>
</plain>
<busses>
</busses>
<nets>
<net name="VDD">
<segment>
<pinref part="V5" gate="G$1" pin="VDD"/>
<pinref part="L2" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="V4" gate="G$1" pin="VDD"/>
<pinref part="U$2" gate="G$1" pin="VDD"/>
<pinref part="C6" gate="G$1" pin="1"/>
<pinref part="C1" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="X2" gate="G$1" pin="VBUS"/>
</segment>
<segment>
<pinref part="V1" gate="G$1" pin="VDD"/>
<pinref part="D1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="_MCLR/VPP/RE3"/>
</segment>
</net>
<net name="VDD_TGT_P">
<segment>
<pinref part="U$2" gate="G$1" pin="KBI0/AN11/RB4"/>
</segment>
</net>
<net name="VPP_FB">
<segment>
<pinref part="U$2" gate="G$1" pin="AN0/RA0"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ICSPAUX">
<segment>
<pinref part="U$2" gate="G$1" pin="RCV/T0CKI/C1OUT/RA4"/>
</segment>
<segment>
<pinref part="ICSP" gate="G$1" pin="6"/>
</segment>
</net>
<net name="MCLR_TGT">
<segment>
<pinref part="U$2" gate="G$1" pin="_SS/HLVDIN/C2OUT/AN4/RA5"/>
</segment>
<segment>
<pinref part="T2" gate="1" pin="G"/>
</segment>
</net>
<net name="OSC2">
<segment>
<pinref part="U$2" gate="G$1" pin="OSC2/CLKO/RA6"/>
</segment>
<segment>
<pinref part="C8" gate="G$1" pin="2"/>
<pinref part="Q1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="OSC1">
<segment>
<pinref part="U$2" gate="G$1" pin="OSC1/CLKI/RA7"/>
</segment>
<segment>
<pinref part="C7" gate="G$1" pin="2"/>
<pinref part="Q1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="U$2" gate="G$1" pin="INT0/FLT0/SDI/SDA/AN12/RB0"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="U$2" gate="G$1" pin="INT1/SCK/SCL/AN10/RB1"/>
</segment>
</net>
<net name="VPP_ON">
<segment>
<pinref part="U$2" gate="G$1" pin="INT2/VMO/AN8/RB2"/>
</segment>
</net>
<net name="VDD_TGT_N">
<segment>
<pinref part="U$2" gate="G$1" pin="CCP2/VPO/AN9/RB3"/>
</segment>
</net>
<net name="SWITCH">
<segment>
<pinref part="U$2" gate="G$1" pin="KBI1/PGM/RB5"/>
</segment>
</net>
<net name="PICKIT_PGC">
<segment>
<pinref part="U$2" gate="G$1" pin="KBI2/PGC/RB6"/>
</segment>
</net>
<net name="PICKIT_PGD">
<segment>
<pinref part="U$2" gate="G$1" pin="KBI3/PGD/RB7"/>
</segment>
</net>
<net name="LED_BUSY">
<segment>
<pinref part="U$2" gate="G$1" pin="T1OSO/T13CKI/RC0"/>
</segment>
</net>
<net name="VPP_PUMP">
<segment>
<pinref part="U$2" gate="G$1" pin="_UOE/T1OSI/CCP2/RC1"/>
</segment>
<segment>
<pinref part="T1" gate="1" pin="G"/>
</segment>
</net>
<net name="VDD_TGT_ADJ">
<segment>
<pinref part="U$2" gate="G$1" pin="CCP1/RC2"/>
</segment>
</net>
<net name="VUSB">
<segment>
<pinref part="U$2" gate="G$1" pin="VUSB"/>
</segment>
<segment>
<pinref part="C9" gate="G$1" pin="1"/>
</segment>
</net>
<net name="D-">
<segment>
<pinref part="U$2" gate="G$1" pin="D-/VM/RC4"/>
</segment>
<segment>
<pinref part="X2" gate="G$1" pin="D-"/>
</segment>
</net>
<net name="D+">
<segment>
<pinref part="U$2" gate="G$1" pin="D+/VP/RC5"/>
</segment>
<segment>
<pinref part="X2" gate="G$1" pin="D+"/>
</segment>
</net>
<net name="WP">
<segment>
<pinref part="U$2" gate="G$1" pin="TX/CK/RC6"/>
</segment>
</net>
<net name="FREE_PIN">
<segment>
<pinref part="U$2" gate="G$1" pin="SDO/RX/DT/RC7"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="ICSP" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="T1" gate="1" pin="S"/>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="-"/>
<pinref part="C2" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="U$2" gate="G$1" pin="VSS@0"/>
<pinref part="U$2" gate="G$1" pin="VSS@1"/>
<pinref part="C6" gate="G$1" pin="2"/>
<pinref part="C1" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="GND8" gate="1" pin="GND"/>
<pinref part="C7" gate="G$1" pin="1"/>
<pinref part="C8" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND10" gate="1" pin="GND"/>
<pinref part="X2" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="C9" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="T2" gate="1" pin="S"/>
</segment>
</net>
<net name="PGC">
<segment>
<pinref part="ICSP" gate="G$1" pin="5"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="VREF+/AN3/RA3"/>
</segment>
</net>
<net name="PGD">
<segment>
<pinref part="ICSP" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="VREF-/CVREF/AN2/RA2"/>
</segment>
</net>
<net name="VPP">
<segment>
<pinref part="ICSP" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="T2" gate="1" pin="D"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="L2" gate="G$1" pin="2"/>
<pinref part="D2" gate="G$1" pin="A"/>
<pinref part="T1" gate="1" pin="D"/>
</segment>
</net>
<net name="VPP+">
<segment>
<pinref part="D2" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="C2" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VDD_TGT">
<segment>
<pinref part="ICSP" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="AN1/RA1"/>
</segment>
<segment>
<pinref part="D1" gate="G$1" pin="C"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
